**EVENT SITE MEASUREMENT**

**STRAIGHT TRACK**

|  |  |  |
| --- | --- | --- |
| **Rule Requirement** | | |
| Track | Length | m |
|  | Number of lanes | m |
|  | Width of lanes | m |
|  | The lanes marked by white lines 0.05m in width | YES  NO |
| Inclination | The maximum lateral inclination of the track is less than 1:100 | YES  NO |
|  | The overall downward inclination in the running direction is less than 1:1000 | YES  NO |
| Notes |  | |

|  |  |
| --- | --- |
| **Track Surface** | |
| *See list:* [*https://www.worldathletics.org/about-iaaf/documents/technical-information*](https://www.worldathletics.org/about-iaaf/documents/technical-information) | |
| Product name |  |
| Product manufacturer |  |
| Absolute thickness |  |
| World Athletics Product Certificate number |  |


**Measured Distance to Finish Line**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Start | Lane 1 | Lane 2 | Lane 3 | Lane 4 | Lane 5 | Lane 6 | Lane 7 | Lane 8 |
| 60m |  |  |  |  |  |  |  |  |
| 100m |  |  |  |  |  |  |  |  |
| 110m |  |  |  |  |  |  |  |  |
| Other |  |  |  |  |  |  |  |  |

## **Event Site – Spot Levels**

* The level at the Finish Line is assumed to be 0.000m. Three check-points should be taken in a line: inside lane one, in the centre of the track and outside the outer lane. Levels need to be provided at the start, and at the Finish Line on the straight.
* It is essential that reduced levels (not grades) be provided on each of the runways.
* The sign convention used by World Athletics for inclinations is that an upward inclination in the direction of running is positive.

## **Spot Levels – Straight Track**



0.000